WARNING!

**OPERATIONS WITH THIS EQUIPMENT CAN BE**

**HAZARDOUS. THE FOLLOWING INSTRUCTIONS**

**MUST BE FOLLOWED AT ALL TIMES**

1. **The immediate work area must be marked off and untrained persons**

**must keep out. Remove all tripping hazards.**

1. **Before starting, inspect all of the equipment for vizable signs of damage or deterioration. Do not operate until repaired by a qualified person.**
2. **A risk assessment must be carried out before starting work in order to identify potential hazards such as the presence of lead paint, flammable substances or oxidising agents.**
3. **All operators must use the following PPE:**
* **Eye Protection.**
* **Non-slip and toe capped safety boots.**
* **Ear protection.**
* **Multi-layer body protection such as safety overalls with HI Viz panels.**

**5. Operators are advised to wash thoroughly after use, to remove residue that may contain traces of harmful substances.**

**6. First aid kits must be readily available at every work site.**